D3XX Driver v 1.0.0.6
COMPATIBILITY:
D3XX driver is compatible with the following Windows operating systems:
•	Windows 10 
•	Windows 10 x64 
•	Windows 8.1
•	Windows 8.1 x64
•	Windows 8
•	Windows 8 x64
•	Windows 7
•	Windows 7 x64
PACKAGE CONTENTS:
The files included in this package are:
•	Driver Files
o	Win7
•	amd64
•	ftdibus3.cat
•	ftdibus3.inf
•	ftdibus3.sys
•	wdfcoinstaller01011.dll
•	i386
•	ftdibus3.cat
•	ftdibus3.inf
•	ftdibus3.sys
•	wdfcoinstaller01011.dll
o	Win8
•	amd64
•	ftdibus3.cat
•	ftdibus3.inf
•	ftdibus3.sys
•	wdfcoinstaller01011.dll
•	i386
•	ftdibus3.cat
•	ftdibus3.inf
•	ftdibus3.sys
•	wdfcoinstaller01011.dll

o	Win8.1
•	amd64
•	ftdibus3.cat
•	ftdibus3.inf
•	ftdibus3.sys
•	wdfcoinstaller01011.dll
•	i386
•	ftdibus3.cat
•	ftdibus3.inf
•	ftdibus3.sys
•	wdfcoinstaller01011.dll
o	Win10
•	amd64
•	ftdibus3.cat
•	ftdibus3.inf
•	ftdibus3.sys
•	i386
•	ftdibus3.cat
•	ftdibus3.inf
•	ftdibus3.sys
RELEASES:
1.0.0.6 (October 15, 2015)	
•	Fixed FT_AbortPipe issue.
•	Added FT_ResetDevicePort and FT_CycleDevicePort.
•	Supported Windows 10 “Universal Drivers”.
•	Released together with D3XX library 1.0.0.8.
•	WHQL certified release.

•	Known Issue: BSOD occurs on Windows 7 x64 when another device is plugged/unplugged while FT600DemoStreamerDemoApp is transferring data. This was observed to happen only if machine has jtagserver.exe running from Altera installation.
1.0.0.5 (September 3, 2015)	
•	First release.
•	WHQL certified release.